WEB Config Tool Guide
1  Download this tool from:

http://beseencontrol.com/ikeys/WEBConfigV2.7_EN.exe 
2  Start the Tool
[image: image1.png]TXYWEB Configure- V2.7

Ty WEB Advenced Oplon





【search】: search the controller in the same local NET Area.
【Try WEB】: By this button, can enter the web interface directly.
【Advanced Option】: Can set the “IP address”,“Sub-net mask”,“gateway address”、“date format”and “Language”.
3  Search controller
Click“Search”，To get the controller which is in the local same net area.
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4  Start WEB 
After search the controller, Click the SN number to select one controller, then click “Try WEB”, You can enter Web interface directly, and the WEB state will display as “Enabled”.
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5  Advanced Options
5.1 Set the IP address of Controller
Click “Advanced Option”, Select the controller and then at left side, input new IP address .etc. after that, click “configure”
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After that, the right side will display the new info you set.
5.2 Set Date Format.
Can set Year-Month-Day, Month-Day-Year, Day-Month-Year .etc.
5.3 设置WEB界面语言

Can set to English.
